To be reduced by 67% to column width of76mm S/S Fonts12/12pt > 67% 8/8pt

Fig. 1

Foam insulated Cryostat

Cos � = 0.9, 0.96, 0.98

B1 1-CCDLadder Striplines to front-end electronics

B2-5 2-CCDLadders

Beam pipe

0 20 10 Scale (cm)