Detector type A

Detector type B

Measured after 10 minutes settling time at 1000 V

Leakage current of CDF-L00 Hamamatsu detectors

Bias (volts)

Reverse Current (nA)