C-V of non-irradiated 300 μm thick Hamamatsu detector

Bias (volts)

Capacitance (pF)

Full depletion voltage ≈ 64 volts