Interstrip capacitance (1^{st} and 2^{nd} neighbours each side) for CDF-L00 detectors

Bias (volts)

Interstrip capacitance (pF)