CCE (from 1060 nm laser) after 8 10^{14} 24 GeV/c protons cm^{-2} standard and oxygenated silicon detectors

Bias (V)

CCE (arb. unit)

Detector thickness = 200 μm