Measured at -18 Α 2 ^oC

I-V of Hamamatsu Wedge detectors after 3x10^{14} p. cm^2 (detector thickness = 250 μm)

Bias (volts)

Reverse Current (μA)

Measured at -10 Α 0.5 ^oC

Bias (volts)

Reverse Current (μA)