Fluence (cm^{-2})

Full depletion voltage (V)

Detector thickness = 300 μm