Strip number

Current (A)

Strip integrity of Hamamatsu stx-41618-12 after 3x10^{14} p. cm^2 (biased to 350 volts during irradiation)

3 pin-holes in total