Strip number

Current (A)

Strip integrity of non-irradiated p-type detector 1728-25

2 pin-holes for 5 volts applied 6 pin-holes for 50 volts applied