Strip number

Current (A)

Strip integrity of non-irradiated p-type detector 1729-7

55 pin-holes in total