Current (A)

Strip integrity of Micron 1732-2-1 after 3x10^{14} p. cm^2

Strip number

Capacitance (F)

2 pin-holes in total 12 strips shorted without evidence of defects in the fan in