Noise vs bias for the non-irradiated and irradiated (3 10^{14} p cm^{-2}) region of LHCb detector

Bias/V_{FD}

Noise counts

The bias is normalised to the full depletion voltage