Charge collection efficiency for the non-irradiated and irradiated (3 10^{14} p cm^{-2}) region of LHCb detector

Bias (V)

CCE

Signal from ^{106}Ru source Electronics: SCT128, 40MHz

CCE is normalised to the plateau value of the non-irradiated region