Charge collection efficiency of oxygenated Micron barrel detectors after 3 10^{14} p cm^{-2} (111 silicon)

Bias (volts)

CCE (arbitrary units)

Charge induced by pulsed 1064 nm laser