Charge collection efficiency of ATLAS wedge detectors after 3 10^{14} p cm^{-2}

Bias (volts)

CCE

Source (^{106}Ru) measurements