Measured at -18 Α 2 ^oC

I-V of Micron miniature detectors after 3x10^{14} p cm^2

(Irradiation in the -20 ^oC box)

Bias (volts)

Reverse Current (μA)

SQRT(Bias) (volts^{1/2})

Reverse Current (μA)

(Shuttle irradiation)