Cross- section of wired version CCD 58 motherboard.

This is an idealistic drawing of the cross section of the cables. In practise it may not be possible to group them as tight as this so it would be wise to allow a reasonable (5- 10mm) margin around them which can be sealed will a semi- flexible material.

This schematic shows the cables only and does not show the connectors on the end. There are 2 25 way D connectors with shrouds which are 55mm x 14mm x 55m. The cable is 1m long and fairly stiff so you should allow for about a 30mm bend radius.