AND SHIELD

and foil if possible for lowest Z ay HF
short between modules using cooling tube

LOWEST VOLTAGE BETWEEN MODULES

V(n)

CpCpCpR
patch panel

HYBRID GROUND PLANE
agnd
dgnd
outoutAMPAMPSHAP

SHAP

COMP

LOGIC

+-