INPUT LOOP - MAGNETIC

to frequency proximity
loop area and current.

N.B. coupling proportional
due to nearby noise current flow
so fairly insensitive to mag fields

Input loop area (shaded) is small

AMPSHAP

COMP

+-