IMPORTANT!!!

inside.

the vac tank and female numbering
male numbering is used outside

Feedthru has pins both sides

Development boards will be

B-SK1

FT1A-SK1

A-PL1

K-SK1

K-PL1

H-SK1

Tony Smith Oct’01  Rev 1.0

PROPOSED VELO HYBRID CONNECTIONS

adapter pcb

Buffer card pcb
are for MALE part
parts. Note pin numbers
fitted with 50 pin male
in experiment

50 way female cannon used

50 way female cannon
feedthrough

50 pin cannon vacuum
in this view
pin1 this side and at far end

FCI 61082 101000 receptacle

FCI 61083 101000 plug
flexible KAPTON double sided PTH - transmission line geometry for signals

Large pin nearest in this view
small pin nearest