122mm
prototype cables will be straight and plug directly into the hybrid

Prototype hybrid will not have tails

Tony Smith Oct ’01

VELO HYBRID V1.0
and orientation

Proposed connector definitions

View A-A

Astraight rather than right angled

Prototype Kapton cables can be
feedthru
to avoid need for a
adapter pcb for prototypes

Fit male cannon to
as a male

Female cannon numbered
a female on inside
a male on outside

Feedthrough numbered as

Numbered as a female

Female cannon

side
solder
adapter pcb1
adapter pcb 2
component

View from Z = 0

Kapton 2 signals only)

Kapton 1 (power and signals)

Solder side of buffer card

B-SK4

FT4A-SK4

B-SK3

FT3A-SK3

A-PL3

K-SK3

K-PL3

H-SK3

B-SK2

FT2A-SK2

B-SK1

FT1A-SK1

A-PL1

K-SK1

K-PL1

H-SK1
hybrid