

%**********************************************************************
%                                                                    **
%     Program  :   PC-INSERT 8.7                                     **
%     Date     :   Jun 24 2005                                       **
%     Time     :   11:41:27 AM                                       **
%     File In  :   k5-0.pcb                                          **
%     File Out :   k5-0.ins                                          **
%     Format   :   AUTO INSERTION FILE                               **
%                                                                    **
%**********************************************************************


$FORMAT
  REFDES       CENTX       CENTY ANGLE      TYPE
        VALUE
$UNITS
         CMM
$BOARD-EXTENT
                   -8750         200       48750      -56500
$BOARD-ORIGIN
                   -8750      -10300
$TARGET
$THROUGH-TOP

     
$THROUGH-BOTTOM


$SMD-TOP
 
      U1    15083.75     9780.64    85  b13outln  custom die ** not loaded**
      U2    14856.91     8541.66    74  b13outln  custom die ** not loaded**
      U3    14390.18     7371.78    63  b13outln  custom die ** not loaded**
      U4    13701.81     6316.81    51  b13outln  custom die ** not loaded**
      U5    12818.97     5418.47    40  b13outln  custom die ** not loaded**
      U6    11776.21     4711.79    28  b13outln  custom die ** not loaded**
      U7    10614.65     4224.71    17  b13outln  custom die ** not loaded**
      U8     9379.82     3976.28     6  b13outln  custom die ** not loaded**
      U9     8120.16     3976.26   354  b13outln  custom die ** not loaded**
     U10     6885.36     4224.72   343  b13outln  custom die ** not loaded**
     U11     5723.79     4711.79   332  b13outln  custom die ** not loaded** 
     U12     4681.03     5418.46   320  b13outln  custom die ** not loaded**
     U13     3798.17     6316.85   309  b13outln  custom die ** not loaded**
     U14     3109.84     7371.77   297  b13outln  custom die ** not loaded**
     U15     2643.12     8541.67   286  b13outln  custom die ** not loaded**
     U16     2416.27     9780.63   275  b13outln  custom die ** not loaded**

 
     CX1    16389.85     9870.60    85     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
     CX2    16001.24     9903.28    85     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
     CX3       16156     8380.86    74     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
     CX4    15780.20     8487.87    74     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
     CX5    15634.16     6964.80    63     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
     CX6    15287.19     7142.92    63     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
     CX7    14834.05     5660.40    51     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
     CX8    14531.29     5906.44    51     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
     CX9    13804.52     4558.46    40     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX10    13555.58     4856.89    40     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX11    12561.86     3665.57    28     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX12    12379.01     4010.13    28     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX13    11186.33     3048.05    17     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX14    11072.43     3421.44    17     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX15     9716.10     2711.64     6     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX16     9675.24     3099.93     6     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX17     8185.79     2669.80   354     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX18     8227.60     3057.62   354     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX19     6701.10     2930.23   343     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX20        6815     3303.63   343     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX21     5295.21     3476.60   332     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX22     5479.27     3820.68   332     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX23     4005.60     4298.31   320     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX24     4256.45     4597.69   320     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX25     2921.20     5346.85   309     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX26     3223.95     5591.46   309     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX27     2050.89     6603.95   297     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX28     2397.62     6781.76   297     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX29     1457.62     7991.28   286     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX30     1831.97     8099.41   286     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX31     1145.96        9465   275     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR
    CX32     1535.67     9501.15   275     cap4x  0.1uF 10v X7R array W3A4YC104MA-MR

      C1       15240       10225   175   cap0603 0.1uF 10v X7R  
      C2       15165        9315   175   cap0603 0.1uF 10v X7R  
      C3    15097.78     8941.01   164   cap0603 0.1uF 10v X7R  
      C4    14843.57     8068.35   164   cap0603 0.1uF 10v X7R  
      C5    14703.66     7721.79   153   cap0603 0.1uF 10v X7R  
      C6    14294.26     6915.19   153   cap0603 0.1uF 10v X7R  
      C7    14082.44     6598.60   141   cap0603 0.1uF 10v X7R  
      C8    13513.23     5890.94   141   cap0603 0.1uF 10v X7R  
      C9    13245.68     5618.90   130   cap0603 0.1uF 10v X7R  
     C10    12548.86     5035.30   130   cap0603 0.1uF 10v X7R  
     C11    12234.36     4820.47   118   cap0603 0.1uF 10v X7R  
     C12    11433.50     4392.94   118   cap0603 0.1uF 10v X7R  
     C13    11084.39     4244.43   107   cap0603 0.1uF 10v X7R  
     C14    10217.37     3977.06   107   cap0603 0.1uF 10v X7R  
     C15     9845.49     3904.98    96   cap0603 0.1uF 10v X7R  
     C16     8943.66     3808.69    96   cap0603 0.1uF 10v X7R  
     C17     8560.46     3809.97    84   cap0603 0.1uF 10v X7R  
     C18     7655.62     3905.75    84   cap0603 0.1uF 10v X7R  
     C19     7286.83     3976.30    73   cap0603 0.1uF 10v X7R  
     C20     6419.46     4240.44    73   cap0603 0.1uF 10v X7R  
     C21     6068.82     4391.38    62   cap0603 0.1uF 10v X7R  
     C22     5268.47     4817.59    62   cap0603 0.1uF 10v X7R  
     C23     4953.71     5034.52    50   cap0603 0.1uF 10v X7R  
     C24     4259.12     5614.96    50   cap0603 0.1uF 10v X7R  
     C25     3990.85     5887.31    39   cap0603 0.1uF 10v X7R  
     C26     3419.70     6592.26    39   cap0603 0.1uF 10v X7R  
     C27     3210.06     6911.14    27   cap0603 0.1uF 10v X7R  
     C28     2797.77     7720.31    27   cap0603 0.1uF 10v X7R  
     C29     2654.25     8072.11    16   cap0603 0.1uF 10v X7R  
     C30     2404.03     8941.59    16   cap0603 0.1uF 10v X7R  
     C31     2338.16     9317.90     5   cap0603 0.1uF 10v X7R  
     C32     2255.99    10221.12     5   cap0603 0.1uF 10v X7R
     C33    16606.46       10154   181    cx1206 2.2uF 10v X7R
     C34    16518.05     9146.77   170    cx1206 2.2uF 10v X7R
     C35    16418.75     8620.09   170    cx1206 2.2uF 10v X7R
     C36    16143.24     7644.91   158    cx1206 2.2uF 10v X7R
     C37    15941.42     7150.27   158    cx1206 2.2uF 10v X7R
     C38    15480.11     6246.84   147    cx1206 2.2uF 10v X7R
     C39    15172.56     5779.11   146    cx1206 2.2uF 10v X7R
     C40    14532.49     4988.44   135    cx1206 2.2uF 10v X7R
     C41    14160.87     4607.85   135    cx1206 2.2uF 10v X7R
     C42    13383.70     3958.14   124    cx1206 2.2uF 10v X7R
     C43    12920.46     3640.33   124    cx1206 2.2uF 10v X7R
     C44       12027     3163.63   112    cx1206 2.2uF 10v X7R
     C45    11532.36     2956.03   112    cx1206 2.2uF 10v X7R
     C46    10565.53     2660.03   101    cx1206 2.2uF 10v X7R
     C47    10040.14     2554.95   101    cx1206 2.2uF 10v X7R
     C48     9032.28     2448.59    90    cx1206 2.2uF 10v X7R
     C49     8468.44     2449.87    90    cx1206 2.2uF 10v X7R
     C50     7460.58     2554.95    78    cx1206 2.2uF 10v X7R
     C51     6936.47     2657.47    78    cx1206 2.2uF 10v X7R
     C52     5968.33     2953.48    67    cx1206 2.2uF 10v X7R
     C53     5474.98     3164.92    67    cx1206 2.2uF 10v X7R
     C54     4582.44     3641.61    56    cx1206 2.2uF 10v X7R
     C55     4115.99     3956.85    56    cx1206 2.2uF 10v X7R
     C56     3340.06     4607.81    45    cx1206 2.2uF 10v X7R
     C57     2964.60     4992.24    45    cx1206 2.2uF 10v X7R
     C58     2328.34     5776.49    33    cx1206 2.2uF 10v X7R
     C59     2019.52     6246.78    33    cx1206 2.2uF 10v X7R
     C60     1558.83     7150.20    22    cx1206 2.2uF 10v X7R
     C61        1357     7644.84    22    cx1206 2.2uF 10v X7R
     C62        1076     8624.27    10    cx1206 2.2uF 10v X7R
     C63      984.19     9149.41    10    cx1206 2.2uF 10v X7R
     C64 **assignment not used**
     C65       16473     8883.45   169    cx1210  ** not loaded** 
     C66    16040.21     7397.18   158    cx1210  ** not loaded** 
     C67    15329.15     6003.24   146    cx1210  ** not loaded** 
     C68    14351.36     4797.81   134    cx1210  ** not loaded** 
     C69    13146.61     3784.74   123    cx1210  ** not loaded** 
     C70    11782.21     3056.98   112    cx1210  ** not loaded** 
     C71       10304     2604.29   101    cx1210  ** not loaded** 
     C72     8741.43        2444    89    cx1210  ** not loaded** 
     C73     7197.77        2603    78    cx1210  ** not loaded** 
     C74     5723.36     3058.21    68    cx1210  ** not loaded** 
     C75     4335.20     3801.97    55    cx1210  ** not loaded** 
     C76     3151.57     4794.51    44    cx1210  ** not loaded** 
     C77     2163.50     6015.30    32    cx1210  ** not loaded** 
     C78     1454.99     7395.11    21    cx1210  ** not loaded** 
     C79     1027.32     8880.06    10    cx1210  ** not loaded** 
     C80 **assignment not used**
     C81        6750        1350   270   cap1206  ** not loaded**       (VCC3 decouple)
     C82        7000        1350   270   cap1206  ** not loaded**       (VCC3 decouple) 
     C83        7250        1350   270   cap1206  ** not loaded**       (VCC3 decouple) 
     C84        7500        1350   270   cap1206  ** not loaded**       (VCC3 decouple) 
     C85        7750        1350   270   cap1206  ** not loaded**       (VCC3 decouple) 
     C86        8000        1350   270   cap1206  ** not loaded**       (VCC3 decouple) 
     C87        8250        1350   270   cap1206  ** not loaded**       (VCC3 decouple) 
     C88        8500        1350   270   cap1206  ** not loaded**       (VCC3 decouple) 
     C89        9000        1350   270   cap1206  ** not loaded**       (VCC1 decouple) 
     C90        9250        1350   270   cap1206  ** not loaded**       (VCC1 decouple) 
     C91        9500        1350   270   cap1206  ** not loaded**       (VCC1 decouple) 
     C92        9750        1350   270   cap1206  ** not loaded**       (VCC1 decouple) 
     C93       10000        1350   270   cap1206  ** not loaded**       (VCC1 decouple) 
     C94       10250        1350   270   cap1206  ** not loaded**       (VCC1 decouple) 
     C95       10500        1350   270   cap1206  ** not loaded**       (VCC1 decouple) 
     C96       10750        1350   270   cap1206  ** not loaded**       (VCC1 decouple) 
     C97        6750         850   270   cap1206  ** not loaded**       (VCC2 decouple) 
     C98        7000         850   270   cap1206  ** not loaded**       (VCC2 decouple) 
     C99        7250         850   270   cap1206  ** not loaded**       (VCC2 decouple) 
    C100        7500         850   270   cap1206  ** not loaded**       (VCC2 decouple) 
    C101        7750         850   270   cap1206  ** not loaded**       (VCC2 decouple) 
    C102        8000         850   270   cap1206  ** not loaded**       (VCC2 decouple) 
    C103        8250         850   270   cap1206  ** not loaded**       (VCC2 decouple) 
    C104        8500         850   270   cap1206  ** not loaded**       (VCC2 decouple) 
    C105        8750         850   270   cap1206  ** not loaded**       (VCC2 decouple) 
    C106        9000         850   270   cap1206  ** not loaded**       (VCC0 decouple)
    C107        9250         850   270   cap1206  ** not loaded**       (VCC0 decouple) 
    C108        9500         850   270   cap1206  ** not loaded**       (VCC0 decouple) 
    C109        9750         850   270   cap1206  ** not loaded**       (VCC0 decouple) 
    C110       10000         850   270   cap1206  ** not loaded**       (VCC0 decouple) 
    C111       10250         850   270   cap1206  ** not loaded**       (VCC0 decouple) 
    C112       10500         850   270   cap1206  ** not loaded**       (VCC0 decouple) 
    C113       10750         850   270   cap1206  ** not loaded**       (VCC0 decouple) 
    C114         380        4745     0   cap1206  10nF 500v         (HT FILTER) 
    C115         380        5055     0   cap1206  10nF 500v         (HT FILTER) 

    C116     4954.98     2894.92    67    cx1206  2.2uF 10v X7R    (POR to GND)
    C117     5139.46     2850.45    67   cap0603  0.1uF 10v X7R    (POR to GND)  
    C118     3442.19     5040.06   135    cx1206  ** not loaded**  (VCC3 to VCC2)
    C119     3535.04     5159.12   135   cap0603  0.1uF 10v X7R    (VCC3 to VCC2)
    C120     8760.13     2778.44   180    cx1206  ** not loaded**  (VCC2 to VCC1)
    C121        8750        2950     0   cap0603  0.1uF 10v X7R    (VCC2 to VCC1)
    C122    14092.15     5050.87   225    cx1206  ** not loaded**  (VCC1 to VCC0)
    C123    13991.09     5175.68   225   cap0603  0.1uF 10v X7R    (VCC1 to VCC0) 
            *


     TS1       16890        8630   180      lm50  ** not loaded** 
     TS2        8460        1850     0      lm50  ** not loaded**  
     TS3         630        8610     0      lm50  ** not loaded** 
      
      R1        1060       10070   180   res0603  75R              (TP TERM)
      R2      520.49     9858.05   180   res0603  75R              (TRIG TERM)
      R3         520        9690     0   res0603  75R              (CLOCK TERM)
      R4         520        9520     0   res0603  75R              (RESET TERM)
      R5         540        6075    90   res0603   zero ohm link   (HTRET to GND)
      R6         960        4955   180   res1206  2k4             (HT FILTER) 
      R7         960        4615   180   res1206  2k4             (HT FILTER) 
      R8         960        4275   180   res1206  2k4             (HT FILTER) 
      R9         960        3955   180   res1206  2k4             (HT FILTER) 
     R10     3381.09     2515.63    90   res0603  100R             (sense3+ to VCC3)
     R11     3521.09     2515.63    90   res0603  0 ohm link       (sense3- to GND)
     R12     4461.09     3215.63    90   res0603  ** not loaded**  (ENEDC to vcc2)  
     R13     4461.09     2875.63    90   res0603  ** not loaded**  (ENEDC to GND)   
     R14     4461.09     2475.63    90   res0603  50R              (ENEDCRET to GND)
     R15     4651.09     2475.63    90   res0603  not loaded -PCB error	 (PORRET to GND)
     R16        7320        1890    90   res0603  0 ohm link       (sense2- to GND)
     R17        7500        1890    90   res0603  100R             (sense2+ to VCC2)
     R18     8681.09     1985.63    90   res0603  100R             (sense1+ to VCC1)
     R19     8821.09     1985.63    90   res0603  0 ohm link       (sense1- to GND)
     R20    14441.09     2145.63    90   res0603  50R              (SCLRET to GND)
     R21    15491.09     2155.63    90   res0603  100R             (sense0+ to VCC0)
     R22    15661.09     2155.63    90   res0603  0 ohm link       (sense0- to GND)
     R23    15831.09     2155.63    90   res0603  50R              (SDARET to GND)
     R24    16855.63     1708.91     0   res0603  ** not loaded**  (COMPCLK TERM)
     R25    14561.09     4295.63    90   res0603  ** not loaded**  (SCL to VCC0)  
     R26    14841.09     4295.63    90   res0603  ** not loaded**  (SDA to VCC0)

   RMON1    15251.09     4895.63    90   0603     ** not loaded**    
   RMON2       15245        4900    90   1206     ** not loaded** 
            *
   SENS1     9131.09     2035.63    90   0603 temp sensor Semitek 103KTJ0608-1P
   SENS2    16681.09     8175.63    90   0603 temp sensor Semitek 103KTJ0608-1P


    SK13        3195        1100     0   aht140r amp 177983-6 receptacle (modified)
    SK11       14295        1100     0   amp140r amp 177983-6 receptacle 


The following two connectors are mounted in the cutouts at the side of the assembly.
They are composed of two parts and need to be assembled before being soldered so that they are correctly positioned. The legs of the smaller part have to be spread slightly in order to fit over the edge of the two sides - please ensure that the legs do not slide under the edge of the flexible circuit - Check this before soldering on either side.  


    SAM1       17025        2800   270       10 pin connector assembly - side mount
    SAM2         475        2800    90       10 pin connector assembly - side mount

$SMD-BOTTOM
$END
